CONSOLIDATED CHECKLIST C6
	Part 3 of 5 parts

	Interim Status Standards for Owners and Operators of
	Hazardous Waste Treatment, Storage, and Disposal Facilities
	40 CFR Part 265, Subparts K-R, as of December 31, 2002

Note:   Consolidated Checklist C6 is divided into five separate documents/computer files solely for ease of handling its printed and electronic versions.  Consolidated Checklist C6 remains one checklist; States must adopt all five portions simultaneously to correctly use this Consolidated Checklist.  Note, the prenotes and endnotes associated with each part have been placed with the part to which they apply.  

Note: No final rules affecting 40 CFR Part 265, Subparts K-R, were promulgated between June 30, 2002 and December 31, 2002, therefore, this Consolidated Checklist corresponds to 40 CFR Part 265, Subparts K-R as published on July 1, 2002.

	
FEDERAL REQUIREMENTS	
CHECKLIST
REFERENCE	
FEDERAL RCRA CITATION	
ANALOGOUS STATE CITATION	
STATE ANALOG IS:	
					
EQUIV-ALENT	
LESS
STRIN-
GENT	
MORE STRIN-GENT	
BROADER IN SCOPE	

SUBPART K - SURFACE IMPOUNDMENTS	

APPLICABILITY	

surface impoundments used to treat, store, or dispose of hazardous waste	
*	
265.220	

	

	
DESIGN REQUIREMENTS	

surface impoundment units that must install two or more liners and a leachate collection and removal system between such liners and operate leachate collection and removal systems in accordance with 264.221(c), "construction commences" defined under "existing facility"	
17 H,100	
265.221(a)	

	

	
notify Regional Administrator; Part B application	
17 H	
265.221(b)	

	

H,	
when a replacement surface impoundment unit is exempt from 265.221(a):	
17 H,100	
265.221(c)	

	

	
constructed in compliance with RCRA 3004(o)(1)(A)(i) and (o)(5) design standards	
100	
265.221(c)(1)	

	

	
no reason to believe liner is not functioning as designed	
100	
265.221(c)(2)	

	

	

H,	
Waiver From Double Liner Requirements	

conditions for waiving 265.221(a)	
17 H	
265.221(d)	

	

		
17 H,74	
265.221(d)(1)	

	

		
17 H	
265.221(d)(2)(i)(A)	

	

			
265.221(d)(2)(i)(B)	

	

			
265.221(d)(2)(i)(C)	

	

			
265.221(d)(2)(ii)	

	

	

H	
first permit must honor liner system installed pursuant to 265.221(a), except if leaking	
17 H	
265.221(e)	

	

	
60 cm of freeboard required	
IV B,H15,100	
265.221(f)	

	

H,4	
condition for variance from 60 cm of freeboard	
15,100	
265.221(g)	

	

	
surface impoundments newly subject to RCRA '3005(j)(1) must be in compliance with 265.221(a),(c)&(d) no later than 48 months after additional characteristic or listing promulgation; Part 268 land disposal prohibitions or an extension to an effective date, within the 48-month period, shall not cut short compliance period	
109	
265.221(h)	

	

4	
ACTION LEAKAGE RATE	

proposed action leakage rate to Regional Administrator when submitting 265.221(b) notice; within 60 days of receipt, Regional Administrator will establish action leakage rate or extend review period; when the proposed rate will be approved	
100	
265.222(a)	

	

	
Regional Administrator approval of action leakage rate for 265.221(a) units; definition of action leakage rate; adequate safety margin	
100	
265.222(b)	

	

	
how to determine if action leakage rate has been exceeded; unless another calculation approved, average daily flow rate calculated weekly during active life and closure period, and monthly during post-closure care period	
100	
265.222(c)	

	

	
CONTAINMENT SYSTEM	

protective cover required for earthen dikes	
IV B	
265.223	

	

5	
RESPONSE ACTIONS	

if unit subject to 265.221(a), then must submit a response action plan to the Regional Administrator when submitting 265.222 proposed action leakage rate; must set forth actions to be taken if action
leakage rate is exceeded; content as specified in 265.223(b)	
100	
265.223(a)	

	

	
responsibilities if flow rate into leak detection system exceeds the action leakage rate for any sump:	
100	
265.223(b)	

	

	
notify Regional Administrator in writing within seven days of determination	
100	
265.223(b)(1)	

	

	
preliminary assessment to Regional Administrator within 14 days of determination; what assessment must address	
100	
265.223(b)(2)	

	

	
determine location, size and cause of any leak	
100	
265.223(b)(3)	

	

	
determine 1) whether waste receipt should cease or be curtailed, 2) whether waste should be removed for inspection, repairs, or controls, and 3) whether unit should be closed	
100	
265.223(b)(4)	

	

	
determine short- and longer-term actions to mitigate or stop any leaks	
100	
265.223(b)(5)	

	

	
within 30 days after Regional Administrator notification, submit the results of 265.223(b)(3)-(5) analyses, the results of actions taken, and actions planned; thereafter, as long as flow rate exceeds action leakage rate, monthly report to Regional Administrator summarizing results of remedial actions taken and actions planned	
100	
265.223(b)(6)	

	

	
how the 265.223(b)(3)-(5) determinations must be made:	
100	
265.223(c)	

	

	
assess the source of liquids and amounts by source	
100	
265.223(c)(1)(i)	

	

	
conduct analyses of liquids in leak detection system to identify sources of liquids and location of leaks, and the hazard and mobility of the liquid	
100	
265.223(c)(1)(ii)	

	

	
assess seriousness of leaks	
100	
265.223(c)(1)(iii)	

	

	
document why assessments not needed	
100	
265.223(c)(2)	

	

	
reserved	
	
265.224	

	

	
WASTE ANALYSIS AND TRIAL TESTS	

waste analyses in addition to 265.13 and the circumstances requiring them	
IV B	
265.225(a)	

	

			
265.225(a)(1)	

	

			
265.225(a)(2)	

	

			
265.225(a)(2)(i)	

	

			
265.225(a)(2)(ii)	

	

	
MONITORING AND INSPECTION	

daily and weekly inspection requirements	
IV B	
265.226(a)	

	

			
265.226(a)(1)	

	

			
265.226(a)(2)	

	

	
if leak detection system required under 265.221(a), record amount of liquid removed from each sump, at least weekly during active life and closure period	
100	
265.226(b)(1)	

	

	
after final cover installed, record amount of liquids at least monthly; when quarterly and semi-annual recording allowed; when monthly recording must resume	
100	
265.226(b)(2)	

	

	
"pump operating level" defined	
100	
265.226(b)(3)	

	

	
reserved	
	
265.227	

	

	
CLOSURE AND POST-CLOSURE CARE	

closure requirements	
IV B,36	
265.228(a)	

	

			
265.228(a)(1)	

	

			
265.228(a)(2)	

	

			
265.228(a)(2)(i)	

	

			
265.228(a)(2)(ii)	

	

			
265.228(a)(2)(iii)	

	

			
265.228(a)(2)(iii)(A)	

	

			
265.228(a)(2)(iii)(B)	

	

			
265.228(a)(2)(iii)(C)	

	

			
265.228(a)(2)(iii)(D)	

	

			
265.228(a)(2)(iii)(E)	

	

	
post-closure requirements	
IV B,36	
265.228(b)	

	

			
265.228(b)(1)	

	

		
100	
265.228(b)(2)	

	

		
IV B,36,100	
265.228(b)(3)	

	

			
265.228(b)(4)	

	

	
removed	
IV B,36	
265.228(c)	

	

	
SPECIAL REQUIREMENTS FOR IGNITABLE OR REACTIVE WASTE	

conditions for placement in a surface impoundment	
*,H15,78	
265.229	

	

	
waste treatment to specific criteria prior to placement	
IV B,H15	
265.229(a)	

	

			
265.229(a)(1)	

	

			
265.229(a)(2)	

	

	
waste management to prevent reaction or ignition	
IV B,H15	
265.229(b)(1)	

	

			
265.229(b)(2)	

	

			
265.229(b)(3)	

	

	
emergency placement	
IV B,H15	
265.229(c)	

	

	
SPECIAL REQUIREMENTS FOR INCOMPATIBLE WASTES	

prohibited co-disposal of incompatible wastes or materials unless compliance with 265.17(b)	
IV B	
265.230	

	

	
AIR EMISSION STANDARDS	

owners/operators subject to applicable requirements of 265, Subparts BB & CC if they place hazardous waste in surface impoundment	
154	
265.231	

	

	
SUBPART L - WASTE PILES	

APPLICABILITY	

storage or treatment facilities using waste piles; alternative management under 265, Subpart N	
IV B	
265.250	

	

	
PROTECTION FROM WIND	

wind dispersal control	
IV B	
265.251	

	

	
WASTE ANALYSIS	

additional analyses	
IV B	
265.252	

	

	
CONTAINMENT	

to control leachate or run-off	
IV B	
265.253	

	

	
place pile on impermeable base with run-on and run-off management	
IV B	
265.253(a)(1)	

	

			
265.253(a)(2)	

	

			
265.253(a)(3)	

	

			
265.253(a)(4)	

	

	
protect pile from precipitation and liquids	
IV B	
265.253(b)(1)	

	

			
265.253(b)(2)	

	

	
DESIGN AND OPERATING REQUIREMENTS	

waste piles which must install two or more liners and a leachate collection and removal system in accordance with 264.251(c) unless exempt under 264.251(d), (e) or (f); compliance with 265.221(b) procedures; "construction commences" defined under "existing facility"	
17 H,100	
265.254	

	

	
ACTION LEAKAGE RATES	

proposed action leakage rate to Regional Administrator when submitting 265.254 notice; within 60 days of receipt, Regional Administrator will establish action leakage rate or extend review period; when the proposed rate will be approved	
IV B	
265.255(a)	

	

	
Regional Administrator approval of action leakage rate for 265.254 units; definition of action leakage rate; adequate safety margin	
100	
265.255(b)	

	

	
how to determine if action leakage rate has been exceeded; unless another calculation approved, average daily flow rate calculated weekly during active life and closure period	
100	
265.255(c)	

	

	
SPECIAL REQUIREMENTS FOR IGNITABLE OR REACTIVE WASTE	

conditions for placement of ignitable or reactive waste in waste piles	
IV B,78	
265.256(a)	

	

		
IV B	
265.256(a)(1)	

	

			
265.256(a)(2)	

	

	
SPECIAL REQUIREMENTS FOR INCOMPATIBLE WASTES	

placement in same pile prohibited unless 265.17(b) is complied with	
IV B	
265.257(a)	

	

	
waste separation or protection	
IV B	
265.257(b)	

	

	
base decontamination	
IV B	
265.257(c)	

	

	
CLOSURE AND POST-CLOSURE CARE	

closure requirements	
IV B	
265.258(a)	

	

	
post-closure care if not all contaminated subsoils can be practically removed	
IV B	
265.258(b)	

	

	
RESPONSE ACTIONS	

if unit subject to 265.254, then must submit a response action plan to the Regional Administrator when submitting 265.255 proposed action leakage rate; must set forth actions to be taken if action leakage rate is exceeded; content as specified in 265.259(b)	
100	
265.259(a)	

	

	
responsibilities if flow rate into leak detection system exceeds the action leakage rate for any sump:	
100	
265.259(b)	

	

	
notify Regional Administrator in writing within seven days of determination	
100	
265.259(b)(1)	

	

	
preliminary assessment to Regional Administrator within 14 days of determination; what assessment must address	
100	
265.259(b)(2)	

	

	
determine location, size and cause of any leak	
100	
265.259(b)(3)	

	

	
determine 1) whether waste receipt should cease or be curtailed, 2) whether waste should be removed for inspection, repairs, or controls, and 3) whether unit should be closed	
100	
265.259(b)(4)	

	

	
determine short- and longer-term actions to mitigate or stop any leaks	
100	
265.259(b)(5)	

	

	
within 30 days after Regional Administrator notification, submit the results of 265.259(b)(3)-(5) analyses, the results of actions taken and actions planned thereafter, as long as flow rate exceeds action leakage rate, monthly report to Regional Administrator summarizing results of remedial actions taken and actions planned	
100	
265.259(b)(6)	

	

	
how the 265.259(b)(3),(4) & (5) determinations must be made:	
100	
265.259(c)	

	

	
assess the source of liquids and amounts by source	
100	
265.259(c)(1)(i)	

	

	
conduct analyses of liquids in leak detection system to identify sources of liquids and location of leaks, and the hazard and mobility of the liquid	
100	
265.259(c)(1)(ii)	

	

	
assess seriousness of leaks	
100	
265.259(c)(1)(iii)	

	

	
document why assessments not needed	
100	
265.259(c)(2)	

	

	
MONITORING AND INSPECTION	

if leak detection system required under 265.254, record amount of liquids removed from each sump, at least weekly during active life and closure period	
100	
265.260	

	

	
SUBPART M - LAND TREATMENT	

APPLICABILITY	

facilities that treat or dispose of hazardous waste in land treatment units	
*	
265.270	

	

	
reserved	
	
265.271	

	

	
GENERAL OPERATING REQUIREMENTS	

conditions for land treatment	
IV B,H15	
265.272(a)	

	

	
run-on control	
IV B	
265.272(b)	

	

	
run-off control	
IV B	
265.272(c)	

	

	
maintenance of collection capacity	
IV B	
265.272(d)	

	

	
wind dispersal control	
IV B	
265.272(e)	

	

	
WASTE ANALYSIS	

additional analyses	
*	
265.273	

	

	
Toxicity Characteristic	
IV B,74	
265.273(a)	

	

	
listed wastes	
IV B	
265.273(b)	

	

	
heavy metals	
IV B	
265.273(c)	

	

	
reserved	
	
265.274 & 265.275	

	

	
FOOD-CHAIN CROPS	

notification if grow food chain crops	
IV B	
265.276(a)	

	

	
prohibition against food chain crops, unless demonstration for 265.273(b) waste constituents	
IV B	
265.276(b)(1)	

	

			
265.276(b)(1)(i)	

	

			
265.276(b)(1)(ii)	

	

	
demonstration information must be kept at facility; what it must be based on; what it must include	
IV B	
265.276(b)(2)	

	

			
265.276(b)(2)(i)	

	

			
265.276(b)(2)(ii)	

	

	
additional requirements for land treatment facility receiving waste with cadmium	
IV B	
265.276(c)	

	

	
requirements if crops are in human food chain	
IV B	
265.276(c)(1)(i)	

	

			
265.276(c)(1)(ii)	

	

			
265.276(c)(1)(iii)	

	

			
265.276(c)(1)(iii)(A)	

	

			
265.276(c)(1)(iii)(B)	

	

	
requirements if crops will be used as animal feed	
IV B	
265.276(c)(2)(i)	

	

			
265.276(c)(2)(ii)	

	

			
265.276(c)(2)(iii)	

	

			
265.276(c)(2)(iv)	

	

	
reserved	
	
265.277	

	

	
UNSATURATED ZONE (ZONE OF AERATION) MONITORING	

written unsaturated zone monitoring plan required and implemented; what plan must be designed to do	
IV B	
265.278(a)	

	

			
265.278(a)(1)	

	

			
265.278(a)(2)	

	

	
what unsaturated zone monitoring must at a minimum include	
IV B	
265.278(b)	

	

			
265.278(b)(1)	

	

			
265.278(b)(2)	

	

	
demonstration required to comply with 265.278(a)(1)	
IV B	
265.278(c)	

	

			
265.278(c)(1)	

	

			
265.278(c)(2)	

	

			
265.278(c)(2)(i)	

	

			
265.278(c)(2)(ii)	

	

			
265.278(c)(3)	

	

	
retention of plan; rationale	
IV B	
265.278(d)	

	

	
soil and soil-pore water analysis	
IV B	
265.278(e)	

	

	
RECORDKEEPING	

operating record to include waste application dates and rates	
IV B	
265.279	

	

	
CLOSURE AND POST-CLOSURE	

objectives which must be addressed in closure and post-closure plans	
IV B	
265.280(a)	

	

			
265.280(a)(1)	

	

			
265.280(a)(2)	

	

			
265.280(a)(3)	

	

			
265.280(a)(4)	

	

	
factors needed to meet the closure and post-closure care objectives of 265.280(a)	
IV B	
265.280(b)	

	

			
265.280(b)(1)	

	

			
265.280(b)(2)	

	

			
265.280(b)(3)	

	

			
265.280(b)(4)	

	

			
265.280(b)(5)	

	

			
265.280(b)(6)	

	

			
265.280(b)(7)	

	

	
methods to address closure/post-closure plan objectives	
IV B	
265.280(c)	

	

			
265.280(c)(1)	

	

			
265.280(c)(2)	

	

			
265.280(c)(2)(i)	

	

			
265.280(c)(2)(ii)	

	

			
265.280(c)(3)	

	

	
closure requirements in addition to Subpart G requirements	
IV B	
265.280(d)	

	

			
265.280(d)(1)	

	

			
265.280(d)(2)	

	

			
265.280(d)(3)	

	

			
265.280(d)(4)	

	

	
certification that facility has been closed in accordance with specifications of approved plan	
IV B	
265.280(e)	

	

	
requirements in addition to 265.117 requirements	
IV B	
265.280(f)	

	

			
265.280(f)(1)	

	

			
265.280(f)(2)	

	

			
265.280(f)(3)	

	

			
265.280(f)(4)	

	

	
SPECIAL REQUIREMENTS FOR IGNITABLE OR REACTIVE WASTE	

conditions for applying ignitable or reactive wastes to treatment zone	
*,78	
265.281	

	

	
immediate incorporation of waste into soil	
IV B	
265.281(a)	

	

			
265.281(a)(1)	

	

			
265.281(a)(2)	

	

	
protective management so no reaction or ignition	
IV B	
265.281(b)	

	

	
SPECIAL REQUIREMENTS FOR INCOMPATIBLE WASTES	

conditions for disposal of incompatible wastes or materials	
IV B	
265.282	

	

	
SUBPART N - LANDFILLS	

APPLICABILITY	

apply to hazardous waste disposal facilities using landfills	
IV B	
265.300	

	

	
DESIGN AND OPERATING REQUIREMENTS	

landfills which must install two or more liners and a leachate collection and removal system above and between such liners, and operate in accordance with 264.301(d), (e) or (f); "construction commences" defined under "existing facility"	
17 H,100	
265.301(a)	

	

	
notify Regional Administrator	
17 H	
265.301(b)	

	

H,	
when a landfill owner/operator is exempt from 265.301(a)	
17 H,100	
265.301(c)	

	

	
meets RCRA 3004(o)(1)(A)(i) and (o)(5) design standards	
100	
265.301(c)(1)	

	

	
no reason to believe liner is not functioning as designed	
100	
265.301(c)(2)	

	

	

H,3	
Waiver From Double Liner Requirements	

waiver for monofills	
17 H	
265.301(d)	

	

		
17 H,108	
265.301(d)(1)	

	

		
17 H	
265.301(d)(2)(i)(A)	

	

			
265.301(d)(2)(i)(B)	

	

			
265.301(d)(2)(i)(C)	

	

			
265.301(d)(2)(ii)	

	

	

H	
liner systems installed pursuant to 265.301(a) will be honored, unless leaking	
17 H	
265.301(e)	

	

	
run-on control	
IV B,100	
265.301(f)	

	

14	
run-off control	
IV B,100	
265.301(g)	

	

14	
collection and holding facilities	
IV B,100	
265.301(h)	

	

14	
wind dispersal control	
IV B,100	
265.301(i)	

	

14	
ACTION LEAKAGE RATE	

proposed action leakage rate to Regional Administrator when submitting 265.301(b) notice; within 60 days of receipt Regional Administrator will establish action leakage rate or extend the review period; when the proposed rate will be approved	
100	
265.302(a)	

	

	
Regional Administrator approval of action leakage rate for units subject to 265.301(a); definition of action leakage rate; adequate safety margin	
100	
265.302(b)	

	

	
how to determine if action leakage rate has been exceeded; unless another calculation approved, average daily flow rate calculated weekly during active life and closure period, and monthly during post-closure care period	
100	
265.302(c)	

	

	
RESPONSE ACTIONS	

if unit subject to 265.301(a), then must submit a response action plan to the Regional Administrator when submitting 265.302 proposed action leakage rate; must set forth actions to be taken if action leakage rate is exceeded; content as specified in 265.303(b)	
100	
265.303(a)	

	

	
responsibilities if flow rate into leak detection system exceeds the action leakage rate for any sump:	
100	
265.303(b)	

	

	
notify Regional Administrator in writing within seven days of determination	
100	
265.303(b)(1)	

	

	
preliminary assessment to Regional Administrator within 14 days of determination; what assessment must address	
100	
265.303(b)(2)	

	

	
determine location, size and cause of any leak	
100	
265.303(b)(3)	

	

	
determine 1) whether waste receipt should cease or be curtailed, 2) whether waste should be removed for inspection, repairs, or controls, and 3) whether unit should be closed	
100	
265.303(b)(4)	

	

	
determine short- and longer-term actions to mitigate or stop any leaks	
100	
265.303(b)(5)	

	

	
within 30 days after Regional Administrator notification, submit the results of 265.303(b)(3)-(5) analyses, the results of actions taken and actions planned; thereafter, as long as flow rate exceeds action leakage rate, monthly report to Regional Administrator summarizing results of remedial actions taken and actions planned	
100	
265.303(b)(6)	

	

	
how the 265.303(b)(3)-(5) determinations must be made:	
100	
265.303(c)	

	

	
assess the source of liquids and amounts by source	
100	
265.303(c)(1)(i)	

	

	
conduct analyses of liquids in leak detection system to identify sources of liquids and location of leaks, and the hazard and mobility of the liquid 	
100	
265.303(c)(1)(ii)	

	

	
assess seriousness of leaks	
100	
265.303(c)(1)(iii)	

	

	
document why assessments not needed	
100	
265.303(c)(2)	

	

	
MONITORING AND INSPECTION	

if leak detection system required under 265.301(a), record amount of liquids removed from each sump, at least weekly during active life and closure period	
100	
265.304(a)	

	

	
after final cover installed, record amount of liquid at least monthly; when quarterly and semiannual recording allowed; when monthly recording must resume	
100	
265.304(b)	

	

	
definition of "pump operating level"	
100	
265.304(c)	

	

	
reserved	
	
265.305-265.308	

	

	
SURVEYING AND RECORDKEEPING	

items which must be in operating record	
*	
265.309	

	

	
location and dimensions of landfill to be shown on maps	
IV B	
265.309(a)	

	

	
contents of each cell and location of each hazardous waste type in each cell	
IV B	
265.309(b)	

	

	
CLOSURE AND POST-CLOSURE CARE	

cover requirements at final closure	
IV B,15	
265.310(a)	

	

			
265.310(a)(1)	

	

			
265.310(a)(2)	

	

			
265.310(a)(3)	

	

			
265.310(a)(4)	

	

			
265.310(a)(5)	

	

	
post-closure requirements	
IV B,15	
265.310(b)	

	

	
final cover requirements	
IV B,15	
265.310(b)(1)	

	

	
maintain and monitor the leak detection system in accordance with 264.301(c)(3)(iv) & (4), and 265.304(b); comply with other applicable Part 265 leak detection system requirements	
100	
265.310(b)(2)	

	

16	
ground-water monitoring system requirements	
IV B,15,100	
265.310(b)(3)	

	

16	
run-on and run-off control requirements	
IV B,15,100	
265.310(b)(4)	

	

16	
protect and maintain surveyed benchmarks	
IV B,15,100	
265.310(b)(5)	

	

	
removed	
IV B,15	
265.310(c)	

	

			
265.310(d)	

	

	
reserved	
	
265.311	

	

	
SPECIAL REQUIREMENTS FOR IGNITABLE OR REACTIVE WASTE	

placement prohibited unless waste and landfill meet Part 268 requirements and waste is no longer ignitable or reactive and 265.17(b) is complied with	
IV B,78	
265.312(a)	

	

		
IV B	
265.312(a)(1)	

	

			
265.312(a)(2)	

	

	
containerized wastes	
IV B,78	
265.312(b)	

	

	
SPECIAL REQUIREMENTS FOR INCOMPATIBLE WASTES	

conditions for disposal in landfill	
IV B	
265.313	

	

	
SPECIAL REQUIREMENTS FOR BULK AND CONTAINERIZED LIQUIDS	

bulk liquid disposal prior to May 8, 1985 only if:	
IV B,17 F	
265.314(a)	

	

	
liner and leachate system requirements	
IV B	
265.314(a)(1)	

	

	
liquids must be stabilized	
IV B,118	
265.314(a)(2)	

	

	
May 8, 1985 free liquids ban	
17 F,118	
265.314(b)	

	

18	
conditions for placement of containers holding free liquids in a landfill	
IV B,H17 F	
265.314(c)	

	

			
265.314(c)(1)	

	

			
265.314(c)(1)(i)	

	

		
IV B,H17 F,118	
265.314(c)(1)(ii)	

	

		
IV B,H17 F	
265.314(c)(1)(iii)	

	

			
265.314(c)(2)	

	

			
265.314(c)(3)	

	

			
265.314(c)(4)	

	

	
paint filter test	
16,H17 F,25,126	
265.314(d)	

	

18	
compliance date	
IV B,H17 F	
265.314(e)	

	

	
sorbents used to treat free liquids disposed in landfills must be nonbiodegradable; definition of nonbiodegradable sorbents	
118	
265.314(f)	

	

20,	
nonbiodegradable sorbents	
118	
265.314(f)(1)	

	

			
265.314(f)(1)(i)	

	

			
265.314(f)(1)(ii)	

	

			
265.314(f)(1)(iii)	

	

20	
tests for nonbiodegradable sorbents	
118	
265.314(f)(2)	

	

	
ASTM Method G21-70 (1984a)	
118	
265.314(f)(2)(i)	

	

	
ASTM Method G22-76 (1984b)	
118,H145	
265.314(f)(2)(ii)	

	

H	
OECD test 301B	
145	
265.314(f)(2)(iii)	

	

20	
nonhazardous liquids ban effective November 8, 1985; what must be demonstrated to Regional Administrator for exemption	
17 F,118	
265.314(g)	

	

H,20	
only reasonable available alternative	
17 F,118	
265.314(g)(1)	

	

H,20	
not a risk of contaminating underground source of drinking water	
17 F,118	
265.314(g)(2)	

	

	
SPECIAL REQUIREMENTS FOR CONTAINERS	

requirements if containers not very small	
15	
265.315	

	

	
at least 90% full	
IV B,15	
265.315(a)	

	

	
crushed, shredded or reduced in volume before burial	
IV B,15	
265.315(b)	

	

	
DISPOSAL OF SMALL CONTAINERS OF HAZARDOUS WASTE IN OVERPACKED DRUMS (LAB PACKS)	

conditions for placement of overpacked drums in landfills	
*	
265.316	

	

	
inside container requirements including DOT requirements	
IV B	
265.316(a)	

	

	
overpacking--DOT requirements; outer container	
IV B,118	
265.316(b)	

	

	
absorbent material	
IV B,118	
265.316(c)	

	

	
incompatible wastes	
IV B	
265.316(d)	

	

	
reactive wastes	
IV B	
265.316(e)	

	

H,	
disposal in compliance with Part 268; fiber drums allowed for incineration of lab packs	
78	
265.316(f)	

	

	
SUBPART O - INCINERATORS	

APPLICABILITY	

regulations apply to owners and operators of hazardous waste incinerators (as defined in 260.10), except as 265.1 provides otherwise)	
IV B,13,19,85	
265.340(a)	

	

H, , 26	
integration of the MACT standards	
182	
265.340(b) intro	

	

H, 25, 26	
except as provided by 265.340(b)(2) and (b)(3), part 265 standards no longer apply when compliance with MACT requirements of part 63, subpart EEE is demonstrated by conducting performance test and submitting NOC under 63.1207(j) & 63.1210(b)	
182, 197	
265.340(b)(1)	

	

H, 25, 26	
following requirements continue to apply even when MACT compliance is demonstrated: 265.351 and applicable requirements of 265, subparts A-H, BB & CC	
182	
265.340(b)(2)	

	

	
when complying with 270.235(a)(1)(i) to minimize emissions of toxic compounds from startup and shutdown, 265.345 remains in effect	
197	
265.340(b)(3)	

	

25,	
exemptions	
IV B,H182	
265.340(c)	

	

			
265.340(c)(1)	

	

			
265.340(c)(2)	

	

			
265.340(c)(3)	

	

			
265.340(c)(4)	

	

	
WASTE ANALYSIS	

analyze wastes not previously burned	
*	
265.341	

	

	
factors which at a minimum must be analyzed	
IV B	
265.341(a)	

	

			
265.341(b)	

	

			
265.341(c)	

	

	
reserved	
	
265.342-265.344	

	

	
GENERAL OPERATING REQUIREMENTS	

during start-up and shut-down, limit waste feed to steady state	
IV B	
265.345	

	

	
reserved	
	
265.346	

	

	
MONITORING AND INSPECTIONS	

monitoring and inspection requirement	
*	
265.347	

	

	
15-minute monitoring of combustion and emission control instruments; appropriate corrections	
IV B	
265.347(a)	

	

	
daily inspection of incinerator and associated equipment	
IV B	
265.347(b)	

	

	
reserved	
	
265.348-265.350	

	

	
CLOSURE	

remove all hazardous wastes and residues	
IV B	
265.351	

	

	
INTERIM STATUS INCINERATORS BURNING PARTICULAR HAZARDOUS WASTES	

certification to burn dioxins	
14	
265.352(a)	

	

	
certification standards and procedures	
14	
265.352(b)	

	

			
265.352(b)(1)	

	

			
265.352(b)(2)	

	

			
265.352(b)(3)	

	

	
SUBPART P - THERMAL TREATMENT	

OTHER THERMAL TREATMENT	

treatment in other than enclosed devices using controlled flame combustion; which subparts the unit is subject to	
IV B,13,94	
265.370	

	

	
reserved	
	
265.371-265.372	

	

	
GENERAL OPERATING REQUIREMENTS	

waste feed limited to steady state conditions of operation, unless process is non-continuous	
IV B	
265.373	

	

	
reserved	
	
265.374	

	

	
WASTE ANALYSIS	

analyze wastes not previously treated to establish steady state or other appropriate operating conditions	
*	
265.375	

	

	
factors which at a minimum must be analyzed	
IV B	
265.375(a)	

	

			
265.375(b)	

	

			
265.375(c)	

	

	
reserved	
	
265.376	

	

	
MONITORING AND INSPECTIONS	

items requiring monitoring and inspections	
IV B	
265.377(a)	

	

			
265.377(a)(1)	

	

			
265.377(a)(2)	

	

			
265.377(a)(3)	

	

	
reserved	
	
265.378-265.380	

	

	
CLOSURE	

remove all hazardous waste and residues	
IV B	
265.381	

	

	
OPEN BURNING; WASTE EXPLOSIVES	

prohibition on open burning of hazardous wastes except for open burning and detonation of waste explosives; definitions	
IV B	
265.382	

	

	
INTERIM STATUS THERMAL TREATMENT DEVICES BURNING PARTICULAR HAZARDOUS WASTE	

certification to burn dioxins	
14	
265.383(a)	

	

	
certification standards and procedures	
14	
265.383(b)	

	

			
265.383(b)(1)	

	

			
265.383(b)(2)	

	

			
265.383(b)(3)	

	

	
SUBPART Q - CHEMICAL, PHYSICAL, AND BIOLOGICAL TREATMENT	

APPLICABILITY	

applies to owners/operators of facilities which treat by chemical, physical, or biological methods in other than tanks, surface impoundments and land treatment facilities, except as 265.1 provides otherwise	
IV B	
265.400	

	

	
GENERAL OPERATING REQUIREMENTS	

comply with 265.17(b)	
IV B	
265.401(a)	

	

	
placement of wastes	
IV B	
265.401(b)	

	

	
cut-off for continuous feed	
IV B	
265.401(c)	

	

	
WASTE ANALYSIS AND TRIAL TESTS	

requirements in addition to 265.13	
IV B	
265.402(a)	

	

			
265.402(a)(1)	

	

			
265.402(a)(2)	

	

			
265.402(a)(2)(i)	

	

			
265.402(a)(2)(ii)	

	

	
INSPECTIONS	

items to be inspected and frequency of inspection	
IV B	
265.403(a)	

	

			
265.403(a)(1)	

	

			
265.403(a)(2)	

	

			
265.403(a)(3)	

	

			
265.403(a)(4)	

	

	
CLOSURE	

remove all hazardous wastes and residues	
IV B	
265.404	

	

	
SPECIAL REQUIREMENTS FOR IGNITABLE OR REACTIVE WASTE	

ignitable or reactive waste must not be placed in treatment process or equipment unless certain conditions are met	
IV B	
265.405(a)	

	

			
265.405(a)(1)	

	

			
265.405(a)(2)	

	

	
SPECIAL REQUIREMENTS FOR INCOMPATIBLE WASTES	

no treatment of incompatible wastes unless 265.17(b) compliance	
IV B	
265.406(a)	

	

	
no hazardous waste placed in unwashed treatment equipment unless 265.17(b) compliance	
IV B	
265.406(b)	

	

	
SUBPART R - UNDERGROUND INJECTION	

APPLICABILITY	

except as 265.1 provides otherwise:	
*	
265.430	

	

	
owner/operator exclusion	
IV B	
265.430(a)	

	

	
Class I and Class IV wells	
IV B	
265.430(b)